### MP-094 APC lid timeout error

The APC has reported that a station lid was in the open position for an excessive amount of time.

What you should do

1. To clear the error, click Clear error in the XYZ Display window. To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, call your Giddings & Lewis service representative.