### Tech80 Interface

The Tech80 This interface supports the manual Tech80 and Scazon Card interfaces. No machine parameter file is needed from the original system to run this interface.

Before starting PC-DMIS, rename the TECH80.dll to interfac.dll.

The Machine Option dialog box has four tabs for the Tech80 interface:

Connection tab

See the "Tech80 Connection tab" topic.

Axis tab

See the "Assigning the Machine Axes" topic.

Resolution tab

See the "Setting the Axes Scale Factor" topic. Default is X=1000.0, Y=1000.0, Z=1000.0.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).