### Portable Toolbar

Portable toolbar

The Portable toolbar contains several icons that allow you to access various frequently used functions and windows that are helpful when programming or measuring with portable devices. This toolbar will only be available for selection if your version of PC-DMIS is configured to work with portable devices. For information on using PC-DMIS with portable machines, see the "PC-DMIS Portable" documentation.

The available toolbar icons are described in this table:

Icon | Description
| Execute | Executes the measurement process for any currently marked feature(s). See "Execute" in the "Using Advanced File Options" section.
| Execute Feature | Executes the selected feature. See "Execute Feature" in the "Using Advanced File Options" section.
| Execute from Cursor | Executes the part program starting at the selected feature and then working down the Edit window. See "Execute From Cursor" in the "Using Advanced File Options" section.
| Mark | Marks the selected feature with the specified mark color and prepares it for execution. See "Mark" in the "Editing a Part Program" section.
| Mark All | Marks all features in the Edit window. See "Mark All" in the "Editing a Part Program" section.
| Clear Marked | Removes all highlights from currently marked features within the Edit window. See "Clear All" in the "Editing a Part Program" section.
| Edit Dialog | Accesses the dialog box associated with the currently selected command in the Edit window if one exists.
| Import from CAD File | Lets you import a part model from any one of the supported file types. See "Importing CAD Data or Program Data" in the "Using Advanced File Options" section.
| Set Alignment | Links the CAD data to the measured data. See "CAD Equals Part" in the "Creating and Using Alignments" section.
| Leap Frog Alignment | Performs a Leapfrog operation. See "Performing a Leapfrog Operation" in the "Creating and Using Alignments" section.
| Curve Mode | Places PC-DMIS into Curve mode (for use with wire-frame). See "Switching Between Curve and Surface Modes" in the "Editing the CAD Display" section.
| Surface Mode | Places PC-DMIS into Surface mode (for use with surface data). See "Switching Between Curve and Surface Modes" in the "Editing the CAD Display" section.
| Scale to Fit | Enlarges or shrinks the views of the graphic in the Graphics Display window to fit your screen. See "Scaling the Drawing" in the "Editing the CAD Display" section.
| Translate Mode | Places PC-DMIS into translate mode. See "Translate Mode" in the "Editing the CAD Display" section.
| 3D Rotate Mode | Three dimensionally rotates the part for the selected view. See "3D Rotate Mode" in the "Editing the CAD Display"
| Program mode | Uses the probe either in offline or online mode to learn and edit your part program. See "Program Mode" in the "Editing the CAD Display" section.
| Virtual Keyboard | Displays a Virtual Keyboard. See "Using the Virtual Keyboard" in the "Using Other Windows, Editors, and Tools" section.
| Probe Readouts | Displays or hides the Probe Readout window. See "Using the Probe Readout Window" in the "Using Other Windows, Editors, and Tools" section.
| Large Status Window | Displays or hides the Status window. See "Using the Status Window" in the "Using Other Windows, Editors, and Tools" section.
| Report Window | Displays or hides the Report window. See "About the Report Window" in the "Reporting Measurement Results" section.
| Quick Start | Displays or hides the Quick Start interface. See "Using the Quick Start Interface" in the "Using Other Windows, Editors, and Tools" section.
| Auto Circle | Displays the Auto Feature dialog box for the creation of Auto Features. See "Inserting Auto Features" in the "Creating Auto Features" section.
| Location Dimension | Displays the Location Dimension dialog box. See "Dimensioning Location" in the "Dimensioning Features" section.
| Create Views | Saves the view of the part as a separate viewset command which can later be recalled. See "Working with Viewsets" in the "Inserting Report Commands" section.