### MLB-080 Improper probe installed

The function is not compatible with the type of probe installed; for example, a sweep function is not valid when a touch probe is installed. This error may also occur on a system with a probe changer if the system is powered up with a probe mounted or a probe is manually mounted when the system believes that no probe is installed.

Effect

Command is not executed.

What you should do

1. Check the command's definition and correct the part program.

2. Adjust the installed equipment to correct the problem.