### Execute From Start Points'

To begin execution at a specified start point, first set the start point by right-clicking inside Command mode and selecting Set Start Point from the shortcut menu, and then choose the Execute from Start Points menu command.

Important: Be aware that if the current tip for that location in the program does not match the current orientation of the probe head, PC-DMIS will not try and go back to execute the tip command above it in order to change the tip orientation.