#### Scan Done

The Scan Done command button alerts PC-DMIS that the scan is complete. This button is only available when a manual scan is being executed (learned). It is located in the Execution Mode Options dialog box. As you execute the scan, data is gathered by PC-DMIS from the CMM. Simultaneously, PC-DMIS filters (reduces) the data according to the method (Fixed Time, Fixed Distance, Fixed Time / Distance etc.) you provide. Data that does not satisfy the criteria (such as Fixed Time or Distance increments) are excluded and data that satisfy the criteria are kept.

In some earlier versions, a Reduce button was available but in this version that is not used. When you press the Scan Done command button, PC-DMIS stops collecting data and processes the data for finding Nominals, Vector compensation etc.