### MP-008 CPU EPROM checksum error

A checksum error has been detected for the MP-30 DCC board EPROMs. The checksum is continuously recalculated while the MP is on. This error indicates that the DCC board is no longer functioning reliably. Refer to MP Error Codes for additional information.

What you should do

1. To clear the error, power the MP down.

2. Power the MP back up.

3. If the error reoccurs, call your Giddings & Lewis service representative.