### TempComp-202 Gradient temperature limit exceeded

Temperature compensation has been requested but the difference in temperature between a pair or thermistors indicates a temperature gradient that exceeds the configured system limits. Temperature compensation is active but system conditions may preclude achieving the desired system accuracy. The message includes the thermistor numbers and recorded temperatures that caused the warning.

Refer to TempComp Error Codes for additional information.

What you should do

1. If possible, correct the identified problem.

2. If the warning reoccurs and cannot be explained by the environmental conditions, call your Giddings & Lewis service representative.