### Insert Defaults

The Edit | Breakpoints | Insert Defaults menu option allows you to set breakpoints throughout the part program at default locations. Default locations are defined as lines in the Edit window that contain commands which generate motion of the CMM or cause branching to occur as a result of a flow control command (such as IF THEN statements). See the "Branching by Using Flow Control" section for more information.