### Auto-Continue Execution

Auto-Continue Execution: This check box determines whether or not the comment that is displayed during execution closes itself after a specified number of seconds. This is useful for operators who use a measuring device that is not nearby the computer. Marking this check box enables the Execution Delay in Seconds box.

Execution Delay in Seconds: This box lets you specify the amount of seconds to delay execution while the comment is displayed. You can specify any number of seconds greater than 0 and less than 600.

- If you use an execution delay with a movie file and the movie's play time exceeds the delay value, PC-DMIS will wait until the movie finishes playing before continuing.

- If your movie value is shorter than the specified execution delay, the comment will remain displayed until the execution delay counts down to zero.

During execution, a count down timer will appear on the Operator comment's OK button inside parentheses:

In the Yes / No comment it will appear on the Yes button.

Once it reaches zero, execution will continue as if the OK button was clicked for an Operator comment or as if the No button was clicked for a Yes / No comment.