Current Help System: PC-DMIS CMM (View Core Help)

### Step 3: Set the View

View Setup dialog box

To change the views in the Graphics Display window you will use the View Setup dialog box. You can access this dialog box by clicking the View Setup icon
from the Graphics Mode toolbar or by selecting the Edit | Graphics Display Window | View Setup menu option:

1. From the View Setup dialog box, select the desired screen style. For this tutorial, click on the second button (top row, second from left) indicating a horizontally split window.

2. To view the upper part image in the Z+ direction, pull down the Blue drop-down list located in the Views area of the dialog box, and select Z+.

3. To view the lower part image in the Y- orientation, pull down the Red drop-down list and select Y-.

4. Click the Apply button and PC-DMIS will re-draw the Graphics Display window with the requested two views. Since you haven't measured the part yet, nothing will be drawn in the Graphics Display window. The screen will be split, however, according to the views selected in the View Setup dialog box.

Note: All of the display options only affect how PC-DMIS displays the part image. They do not have an effect on the measured data or inspection results.

Go to the next step: "Measure the Alignment Features".