Current Help System: PC-DMIS CMM (View Core Help)

#### Set Move Speed

Parameter Settings Dialog box—Motion tab

The Move Speed option lets you change the point to point positioning speed of the CMM.

1. Access the Parameter Settings dialog box by selecting Edit | Preferences | Parameters.

2. Select the Motion tab.

3. Place your cursor in the Move Speed box.

4. Select the current move speed value.

5. Type 50. This value indicates a percentage of full machine speed.

Based on this setting, PC-DMIS will move the CMM at half of its full speed. The default settings for the other options are satisfactory for this exercise.

See "Parameter Settings: Motion tab" in the "Setting your Preferences" section of the PC-DMIS Core documentation for additional information on Move Speed as well as other motion options.