Current Help System: PC-DMIS Laser (View Core Help)

#### Measurement Properties Area

For information about the specific parameters that are configured in this section, see the following topics:

- Surface Point Specific Parameters

- Edge Point Specific Parameters

- Plane Specific Parameters

- Circle Specific Parameters

- Slot Specific Parameters

- Flush and Gap Specific Parameters

- Cylinder Specific Parameters

- Sphere Specific Parameters

Measure Now: This toggle button determines whether or not PC-DMIS measures the feature when you click Create.

Re-Measure: This toggle button determines whether or not PC-DMIS automatically re-measures the feature a second time once the feature has been measured. It will use the measure values from the first measurement as the target locations for the second measurement.

Auto Wrist: This toggle button will cause the probe orientation to move to a vector that closely corresponds to the surface vector of the Auto Feature.

View Normal: Clicking this button orients that CAD so that you look down on the feature.

View Perpendicular: Clicking this button orients the CAD so that you look at the side of the feature.

Probe Toolbox Toggle: Shows/Hides the Probe Toolbox with the settings for the feature represented in the Auto Feature dialog box.