Current Help System: PC-DMIS Laser (View Core Help)

#### Plane Command Mode Text

The Plane command inside the Edit window’s Command Mode looks like this:

PLN1=FEAT/LASER/PLANE,CARTESIAN,TRIANGLE

THEO/<1.895,1.91,1>,<0,0,1>

ACTL/<1.895,1.91,1>,<0,0,1>

TARG/<1.895,1.91,1>,<0,0,1>

WIDTH=3,LENGTH=7

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,1

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE