Current Help System: PC-DMIS Laser (View Core Help)

#### Filter Type: Weighted Average

This is only available for Perceptron sensors.

Weighted Average Filter Type

The Weighted Average filter smoothes stripe data by computing a new location for each pixel. For each pixel in the stripe, this filter will use a weighted average of its neighboring pixels to compute a new location. This is the default filter.

Neighbor #: This value determines the number of total pixels considered when calculating a new location of any given pixel in a single stripe.

Set Weights: This button sets the relative importance of a given pixel’s neighbor.

Use the up and down arrows for each of the pixel locations. Click OK to save your changes or Cancel to close without saving.