Current Help System: PC-DMIS Laser (View Core Help)

## Pointcloud Operators

The Pointcloud Operator command (COPOPER) performs different operations on Cloud of Point (COP) commands and other COPOPER commands.

Note: The units for COPOPER commands are in millimeters.

Adding Pointcloud Operators to your part program can be done in a variety of different ways:

- Select the Insert | Pointcloud | Operator menu item.

- Select menu items from the following submenus:

- File | Import | Pointcloud: Import from data files to a COP.

- File | Export | Pointcloud: Export to data files from a COP.

- Insert | Pointcloud: Add a basic pointcloud command from this sub-menu. Command include COP, COPOPER and specific COPOPER commands (Cross Section, Face Colormap or Point Colormap) which alter the display of Pointclouds in the Graphics Display window.

- Operation | Pointcloud: Alter the number of points that are included in COP or COPOPER commands. Items is this submenu include: Clean, Empty, Filter, Purge, Reset, and Select.

- Manually type the COPOPER command into the Edit Window. Pressing F9 on the COPOPER command in the Edit Window will open the Pointcloud Operator dialog box.

- Click the needed Pointcloud Operator button from the Pointcloud toolbar to open the associated Pointcloud Operator dialog box. The Pointcloud Operator will be applied to the

Note: Your portlock must be programmed with the COP option to use COPOPER capability. Also, you will not be able to use COPOPER commands if your portlock is programmed with Vision options. Vision should be disabled when using Laser.

More:

Manipulating Pointcloud Operators

Boolean COPOPER

Clean COPOPER

Complement COPOPER

Cross Section COPOPER

Empty COPOPER

Export COPOPER

Face Colormap COPOPER

Filter COPOPER

Import COPOPER

None COPOPER

Point Colormap COPOPER

Purge COPOPER

Reset COPOPER

Select COPOPER