Current Help System: PC-DMIS Portable (View Core Help)

## Using Romer Arm Buttons

There are two types of button configurations that exist:

| Two Button Configuration: 2 Buttons are programmed for use by PC-DMIS (even though 3 buttons exist). The two buttons indicated in the image to the right perform the same function. See "Two Button Configuration"
| Three Button Configuration: 3 Buttons are programmed for use by PC-DMIS. The buttons have color coded dots. See "Three Button Configuration"

Mouse Mode

PC-DMIS lets you place your portable device into "Mouse Mode". This special mode lets you perform standard mouse pointer actions (move the pointer, click or right-click, etc.) inside PC-DMIS by moving the arm and probe head around and pressing buttons to perform mouse "clicks". PC-DMIS interprets the motion as if you were using a standard mouse. This allows you to remain with your portable device rather than continually switching between device and computer.

If PC-DMIS is in Mouse Mode and you attempt to pick up and use your regular mouse, it will behave erratically. You should exit out of this mode prior to using your standard mouse functionality.

Mouse Mode functions outside of PC-DMIS but only if PC-DMIS remains running and minimized in the background.

See the "Two Button Configuration" and "Three Button Configuration" topics for more information on how mouse mode is used.