Current Help System: PC-DMIS Portable (View Core Help)

### Finding a Reflector

The Find function allows you to search in a spiral pattern to find the actual location of a reflector or T-Probe with your Leica Tracker or Total Station device.

Finding a Reflector Location Using a Leica Tracker Device

1. Approximately point the Tracker laser to the location of the desired reflector. This can be done by one or all of the following:

- "Releasing Tracker Motors" and manually moving the laser to the location.

- Using the control buttons on the "ADM" tab of the Machine Options dialog box...

- Using the Overview camera ...

- Using the Alt + left arrow, right arrow, up arrow, down arrow keyboard keys to move the tracker head. Use Alt + Space to stop movement of the laser.

2. Select the Tracker | Find menu item. The tracker device will search in a spiral pattern and take readings until the reflector sends the signal back to the device. This will locate the position.

Finding a Reflector Location Using a Total Station Device

1. Approximately point the Total Station laser to the location of the desired reflector. This can be done by one or all of the following:

- Manually moving the laser to the location...

- Using the Alt + left arrow, right arrow, up arrow, down arrow keyboard keys to move the tracker head. Use Alt + Space to stop movement of the laser.

2. Select the Total Station | Find menu item. The total station device will search in a spiral pattern and take readings until the reflector sends the signal back to the device. This will locate the position.

Note: This function can also be executed from the View Camera dialog box.