Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Pnt Spacer

Allows you to define the default value for the Point Spacer option that will be used when an Auto Feature is created. The Point Spacer value defines the distance from the nominal point location that PC-DMIS will use to measure a point if sample hits are specified.

Entry Name: DccPntSpacer

Entry Type: Real Number to specify distance. Default value is 0.

User permission is required to change entry