Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Rotab Init Timeout

Specifies a timeout for response to the initial attempt to communicate with the table when PC-DMIS is started. A value of 0.0 disables this timeout. If the timeout occurs, the user will be prompted as to whether or not to try resending the command for which the response was not received within the allowed time.

Entry Name: ExternalRotabInitTimeout

Entry Type: Real Number specifying seconds. Default value is 5.

User permission is required to change entry