Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Cal Order

When this value is set to TRUE (1), PC-DMIS allows you define the User Define Calibration. With this value set to TRUE (1) you can then hold down the CTRL key and select the tips from the Active Tip List for calibration with your left mouse button from the Probe Utilities dialog box. A number representing the index of the tip measurement order appears next to each Tip ID as it is selected.

Entry Name: ProbeCalOrder

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry