Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Prb Comp

PC-DMIS uses probe compensation when this value is set to TRUE (1).

Entry Name: ScanDialogPrbComp

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 1.

User permission is required to change entry

Note: In most cases you probably don't need to perform this compensation since a scan's FINDNOM operation automatically does it. However, if you don't have CAD and want to reverse-engineer a part, you should select this check box.