Current Help System: PC-DMIS Settings Editor (View Core Help)

### Offset Along Tip Vector

When this value is set to TRUE (1), PC-DMIS will offset a move point along the active tip's vector. When set to FALSE(0), PC-DMIS will offset the move point along either the CAD's surface vector or along the feature's vector according to the "OffsetFromCAD" value.

Entry Name: OffsetAlongTipVector

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry