Current Help System: PC-DMIS Settings Editor (View Core Help)

### RMS Out Tol Action

Specifies the action that will be taken when the RMS value for a hit is out-of-tolerance.

Entry Name: RMSOutTolAction

Entry Type: Whole Number to specify out-of-tolerance action. Default value is 0.

User permission is required to change entry

Action Key

Value | Action
0 | Accepts the hit.
1 | Rejects the hit.
2 | Prompts the user to accept or reject the hit.