Current Help System: PC-DMIS Settings Editor (View Core Help)

### Compass Active Alignment

Determines when the Vision Compass functionality will be used: Always (0), After Partial Alignment (1), or After Full Alignment (2).

Entry Name: CompassActiveAlignment

Entry Type: Whole Number to specify when Compass will be used. Default value is After Full Alignment (2).

User permission is required to change entry