Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Sphere In Out

This value allows you to define the default value for the In/Out option that will be used when an Auto Feature is created. The In and Out value tells PC-DMIS whether to construct the sphere as an internal or an external sphere.

Entry Name: DCCSphereInOut

Entry Type: Whole Number to specify Internal Sphere (0) or External Sphere (1). Default value is 0.

User permission is required to change entry