Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Auto Move

This option determines whether Auto Moves are used for each scan. When this option set to TRUE (1), the "ScanDialogAutoMoveVal" will define the distance of Auto Move commands. For the applicable scan types, PC-DMIS will add move commands before and after the scan feature.

Entry Name: ScanDialogAutoMove

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry