Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Tool Over (IJK)

These IJK vector values specify a vector used by PC-DMIS to determine the most efficient order to measure all the tips when the "ProbeCalOrder" is set to TRUE (1).

Entry Name: ProbeShankNumHits

Entry Type: Real Number specifying vector values. Default value is 0 for I & J while the value is 1 for K.

User permission is required to change entry