Current Help System: PC-DMIS Settings Editor (View Core Help)

### Point Tolerance Plus

Provides the positive tolerance from the nominal, and is specified in current part program units. Points that are greater than this value from the nominal will be colored based on the standard PC-DMIS plus tolerance color.

Entry Name: PointTolerancePlus

Entry Type: Character String to specify distance. Default value is None ( ).

User permission is required to change entry