Current Help System: PC-DMIS Settings Editor (View Core Help)

### Start Point-(XYZ)

These values indicate the default coordinates of a point belonging to the first plane cutting the pointcloud that is displayed in the Pointcloud Operator dialog box. The start point value is defined with the START PT parameter in the Edit Window.

Entry Name: Start-(XYZ)

Entry Type: Real Number specifying XYZ values. Default values are X=0, Y=0, & Z=0.

User permission is required to change entry

See the "CROSS SECTION" topic of the PC-DMIS Laser help file for more information.