Current Help System: PC-DMIS Settings Editor (View Core Help)

#### EW Report Mode Show Tol Bi Lower Percent

This value is set for the lower percentage of a bilateral dimension.

Entry Name: `EWReportModeShowTolBiLowerPercent`

Entry Type: Whole Number that specifies the percentage used for the lower tolerance. Default value is 0.

User permission is required to change entry

Example of Bilateral Lower Percentage:

Nominal: 3.0000

Measured:2.9925

Deviation:0.0075

Plus Tol: 0.0100

Minus Tol:0.0100

The percentage is calculated using the Lever Rule:

(2.9925-2.9900) / (3.0100-2.9900) * 100. = 12.5.%

This dimension will be displayed in the inspection report if the Bilateral Lower Percentage is less than 12.5%.