Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Ring Face To Hole Focus Offset Auto Update

When this value is set to TRUE (1), "ProbeQualVisionRingFaceToHoleFocusOffset" value will be updated automatically each time the ring is measured with a vision probe. This will allow offsets that create focus failures to be manually adjusted once and then run automatically on subsequent runs.

Entry Name: ProbeQualVisionRingFaceToHoleFocusOffsetAutoUpdate

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.

User permission is required to change entry