Current Help System: PC-DMIS Settings Editor (View Core Help)

### RMEAS Insert Mode To New PP

This value controls the RMEAS insert method for NEW part programs.

Entry Name: RMEASInsertModeToNewPP

Entry Type: Character String to specify RMEAS mode. Default value is NONE.

User permission is required to change entry

Thickness Type Key:

NONE | Adds NO Command to the part program
LEGACY | Adds RMEAS/LEGACY to the part program
DEFAULT | Adds RMEAS/DEFAULT to the part program