Current Help System: PC-DMIS Settings Editor (View Core Help)

### Cur Temp (0-31)

These values store the current readings from your temperature sensors for your master arm. You can have anywhere from 1 to 32 sensors. These values are provided in Celsius or Fahrenheit according to the TempCompCelsius value.

Entry Name: CurTemp(0-31)

Entry Type: Character String to specify temperature. Default value is 0.0.

User permission is required to change entry