Current Help System: PC-DMIS Settings Editor (View Core Help)

### Renishaw Calibration Order SP600

This value is used in conjunction with the "RenishawCalibrationCreateOrderSP25" and "RenishawCalibrationCreateOrderSP80" values to determine the order in which SP600 probe tips will be calibrated.

Entry Name: RenishawCalibrationOrderSP600

Entry Type: Whole Number to specify calibration order. Default value is 0.

User permission is required to change entry