Current Help System: PC-DMIS Settings Editor (View Core Help)

### Perceptron Sensor Type

Specifies the value for the last used sensor type that was configured for use with PC-DMIS. This allows you configure options that are specific for each sensor type while offline.

Entry Name: PerceptronSensorType

Entry Type: Whole Number to specify sensor type. Default value is 0.

User permission is required to change entry

Value Key:

0 | Digital
1 | V4
2 | V4i
3 | V4ix
4 | V5