Current Help System: PC-DMIS Settings Editor (View Core Help)

### Slave Material Coeff (0-3)

The Slave Material Coefficient values provide numbers reflecting the material property, and are the fractional change in length per unit change in temperature.

Example: A scale with a coefficient of 11.5 microns/meter/degree C becomes 0.0000115 meters/meter/degree C or just 0.0000115/degree C.

Note: This can be thought of as meters/meter/degree C or inches/inch/degree F but since the length in both the numerator and denominator are in the same units they divide out.

Entry Name: SlaveMaterialCoeff(0-3)

Entry Type: Character String specifying degrees in either Celsius or Fahrenheit. Default value is 0.0.

User permission is required to change entry

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part