Current Help System: PC-DMIS Settings Editor (View Core Help)

### Enum Tools Type

This value affects the “EnumTools” command and allows the I++ Server to enumerate to the I++ client both calibrated and uncalibrated tools (0) or only calibrated tools (1).

Entry Name: CommPort

Entry Type: Whole Number to specify enumeration. Default value is 0.

Administrator permission is required to change entry