Current Help System: PC-DMIS Settings Editor (View Core Help)

### Exec Coll Window Opt Pos (1-4)

These values store the last position of the Execution Collision detection window for Arms 1-4 respectively. PC-DMIS will restore the last position upon subsequent part program executions. The comma delimited string refers to pixel values for the top left and bottom right corners of the Execution Mode Options dialog box.

Entry Name: ExecCollWindowOptPos(1-4)

Entry Type: Character String specifying Executive window location. Default value is (0,0,300,200).

User permission is required to change entry

Position Key:

1st # | Top left X position from left edge of screen.
2nd # | Top left Y position from top edge of screen.
3rd # | Bottom Right X position from left edge of screen.
4th # | Bottom Right Y position from top edge of screen.