Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Nom Mode

This option determines the nominals method that will be used to gather nominal information.

Entry Name: ScanDialogNomMode

Entry Type: Whole Number specifying Nominal Method number. Default value is 0.

User permission is required to change entry

Nominal Method Key

0 | MASTER | PC-DMIS will consider the measured data obtained the first time the scan is being learned as nominal data. Subsequent executions of this scan will be compared with this measured data.
1 | FINDNOMS | When the FIND NOMS option is selected, PC-DMIS will pierce the CAD model to find the closest location on a CAD surface to the measured point. It will then set the nominals to the location found on the CAD surface.
2 | NOMINALS | PC-DMIS will use any measured data the first time it performs the scan as nominal data. This option allows you to relearn the scan without relearning the nominals.