Current Help System: PC-DMIS Settings Editor (View Core Help)

### Slave Temp Origin (0-3)

The Slave Origin values are used to determine the length of the item to which thermal compensation is being applied for the Slave arm of a dual arm configuration.

Length = Current Position Value – Origin Value

- The X, Y, and Z values of the Origin boxes will be zero most of the time. However, some types of machines do not use zero for the origin of their scales.

- The Part value will typically also be zero unless there is some special type of fixturing constraint.

Entry Name: SlaveTempOrigin(0-3)

Entry Type: Character String specifying origin location. Default value is 0.0,0.0,0.0.

User permission is required to change entry

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part