Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sphere Center (0-99)

These values provide the spheres positions that are measured during the dual arm calibration process. Sphere positions are only used when the DCCMode is set to TRUE (1).

Entry Name: SphereCenter(0-99)

Entry Type: Character String specifying sphere positions. Default value is ” -99.9,-99.9,-99.9”.

User permission is required to change entry