Current Help System: PC-DMIS Settings Editor (View Core Help)

### Flush

Provides the height difference between two mating sheet metal parts of a Flush and Gap Laser Auto Feature. Whether or not the flush value is positive or negative depends on whether it’s higher or lower than the “Master” side.

Entry Name: Flush

Entry Type: Real Number to specify flush distance. Default value is 0.

User permission is required to change entry