Current Help System: PC-DMIS Settings Editor (View Core Help)

### Use Volvo Deviation Letters

When this value is set to TRUE (1), the part program will display F/B/I/O/H/L after the deviation to identify the direction of the error on the car.

Entry Name: UseVolvoDeviationLetters

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry