Current Help System: PC-DMIS Vision (View Core Help)

#### Changing the Magnification of the Part Image

On a machine with a DCC Zoom, these are the several ways you can alter the magnification of the part image:

Use the Magnification tab: You can do this by either moving the slider bar up or down, or by typing a value in the box next to the slider. By default, the software uses the lowest magnification to get the largest FOV.

Drag the Green Handles of the FOV: Use the FOV handles in the CAD View to resize the rectangle. Grab any corner of the green box and drag the outline to its desired location. On a DCC stage, the green boxes on the edges (not the corners) allow you to move the location of the FOV, not change its size.

Zoom in Live View: In Live View hold down the right and left mouse buttons simultaneously. Drag the cursor across the view, creating an outline of a box. When you release the mouse buttons, the field of view magnifies in the requested location.

Use the Magnification menu: Select menu items from the Operation | Magnification sub-menu or....

...Use the Shortcut Menu in Live View: You can also right click within the Live View tab to access the Magnification sub-menu. (Be sure that your cursor isn’t over the target while right clicking.)

Use Shortcut Keys: Use these shortcut keys to alter the magnification in either Cad View or Live View:

Magnify Action | Shortcut Keys
Increase Fine | ALT + *
Increase Coarse | CTRL + *
Increase Maximum | CTRL + ALT + *
Decrease Fine | ALT + /
Decrease Coarse | CTRL + /
Decrease Minimum | CTRL + ALT + /

The numbers displayed next to the top left and bottom right corners of the image in the Field of View box of the Probe Toolbox, indicate the X and Y coordinate values for the FOV. It also displays the current magnification size in pixels.