PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
SetScanHitParams Method
See Also

Collapse All Expand All

htype

INIT_HITS
  Number of init sample hits to use. Optional.

PERM_HITS
  Number of permanent hits. Optional.

Spacer
  Spacer value. Optional.

Depth
  Depth value. Optional.

Indent
  Indent value. Optional.

flags
  For now, just PCD_EXTERIOR or PCD_INTERIOR. Default is PCD_EXTERIOR. Optional.

# Description

Sets scan hit parameters (used in StartScan block)

# Syntax

Visual Basic

    Public Sub SetScanHitParams( _
       ByVal htype As PCDSCANHITTYPE, _
       ByVal INIT_HITS As Long, _
       ByVal PERM_HITS As Long, _
       ByVal Spacer As Double, _
       ByVal Depth As Double, _
       ByVal Indent As Double, _
       ByVal flags As PCDSCANHITFLAG _
    )

# Parameters

htype

  Value | Description
  --- | ---
  PCD_VECTORHIT |
  PCD_SURFACEHIT |
  PCD_EDGEHIT |
  PCD_ANGLEHIT |

INIT_HITS
  Number of init sample hits to use. Optional.
PERM_HITS
  Number of permanent hits. Optional.
Spacer
  Spacer value. Optional.
Depth
  Depth value. Optional.
Indent
  Indent value. Optional.
flags

  Value | Description
  --- | ---
  PCD_EXTERIOR |
  PCD_INTERIOR |

  For now, just PCD_EXTERIOR or PCD_INTERIOR. Default is PCD_EXTERIOR. Optional.

# Remarks

This function is only used for DCC scans and should not be called for manual scans.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.