PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
MoveCmd Object Members
See Also Overview

Collapse All Expand All

# Public Properties

Angle | Read/Write: Rotation Table Angle Represents the rotation angle of this MOVE_ROTAB object.
Direction | Read/Write: Roation Table Move Direction Represents the rotation direction of this MOVE_ROTAB object.
IJK | Read/Write: Gets/Sets IJK data via Point Data Object for Move Command A PointData object that represents the IJK vector to use.
NewTip | Read/Write: Move PH9 Offset New Tip Value Represents the new tip position of this MOVE_PH9_OFFSET object.
OldTip | Read/Write: Move PH9 Offset Old Tip Value Represents the new tip position of this MOVE_PH9_OFFSET object.
Parent | Read Only: Returns Parent Command Object Returns the parent Command object. Read-only.
XYZ | Read/Write: Gets/Sets XYZ data via Point Data Object for Move Command A PointData object that represents the location to which to move, or in the case of MOVE_INCREMENT, the location offset.
XYZEnd | Read Only: Gets XYZ data via Point Data Object for Circular Move Command End Point
XYZStart | Read Only: Gets XYZ data via Point Data Object for Circular Move Command Start Point

# See Also

MoveCmd Overview | MoveCommand Property

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.