PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
LEAPFROG Object Members
See Also Overview

Collapse All Expand All

# Public Properties

full | Read/Write: Full or partial leapfrog Determines whether or not the leapfrog will be full (1) or partial (0). For more information on this, see the "Creating and Using Alignments" topic in the PC-DMIS Help File.
leapfrogtype | Read/Write: Type of Leapfrog to be performed Integer value that defines the type of feature used to translate the CMM along the part.
NumHits | Read/Write: Number of hits Integer value that determines the number of hits used for the feature types described in the LeapFrogType property. The feature type determines if the number of hits are useful or not.

# See Also

LEAPFROG Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.