PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
GetBoundaryConditionParams Method
See Also

Collapse All Expand All

nCrossings
  Required Long variable that gets the number of crossings for this boundary condition. The scan would stop after the probe crosses (breaks) the Boundary Condition like a Sphere, Cylinder, Cone, or a Plane the given number of times.

dRadius
  Required Double variable that gets the radius of the boundary condition. This is used by the Spherical and Cylindrical Boundary Conditions.

dHalfAngle
  Required Double variable that gets the half-angle of the cone-type boundary condition, or gets zero if the boundary condition is not of cone type.

# Description

Gets the boundary condition parameters

# Syntax

Visual Basic

    Public Function GetBoundaryConditionParams( _
       ByRef nCrossings As Long, _
       ByRef dRadius As Double, _
       ByRef dHalfAngle As Double _
    ) As Boolean

# Parameters

nCrossings
  Required Long variable that gets the number of crossings for this boundary condition. The scan would stop after the probe crosses (breaks) the Boundary Condition like a Sphere, Cylinder, Cone, or a Plane the given number of times.
dRadius
  Required Double variable that gets the radius of the boundary condition. This is used by the Spherical and Cylindrical Boundary Conditions.
dHalfAngle
  Required Double variable that gets the half-angle of the cone-type boundary condition, or gets zero if the boundary condition is not of cone type.

# Return Type

Boolean value. This returns true if the function succeeds, false if it fails.

# Remarks

Boundary Condition | GetBoundaryConditionParams(nCrossings, dRadius, dHalfAngle)
--- | ---
Plane | nCrossings
Cone | nCrossings, ,dHalfAngle
Cylinder | nCrossings, dRadius
Sphere | nCrossings, dRadius

# See Also

BasicScan Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.