PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
DCC Property
See Also

Collapse All Expand All

# Description

Gets or sets whether the Master / Slave calibration is a manual (0) or DCC (1) calibration.

# Property type

Read-write property

# Syntax

Visual Basic

    Public Property DCC() As ENUM_MASTERSLAVEDIALOG_MEASUREDCC

# Return Type

Read/write Long.

# Remarks

The available settings are:

MEASURE_MANUAL = 0

MEASURE_DCC = 1

# See Also

MasterSlaveDlg Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.